nvic: IRQControllers.NVIC @ sysbus 0xE000E000
    systickFrequency: 72000000
    priorityMask: 0xF0
    IRQ -> cpu@0

cpu: CPU.CortexM @ sysbus
    cpuType: "cortex-m7"
    nvic: nvic

itcm: Memory.MappedMemory @ sysbus 0x0
    size: 0x80000

dtcm: Memory.MappedMemory @ sysbus 0x20000000
    size: 0x80000

ocram2: Memory.MappedMemory @ sysbus 0x20200000
    size: 0x80000

wdog1: Python.PythonPeripheral @ sysbus 0x400B8000
    size: 0x4000
    initable: true
    filename: "scripts/pydev/ticker.py"

trng: Miscellaneous.IMX_TRNG @ sysbus 0x400CC000

wdog2: Python.PythonPeripheral @ sysbus 0x400D0000
    size: 0x4000
    initable: true
    filename: "scripts/pydev/ticker.py"

wdog3: Python.PythonPeripheral @ sysbus 0x400BC000
    size: 0x4000
    initable: true
    filename: "scripts/pydev/ticker.py"

iomuxc: Python.PythonPeripheral @ sysbus 0x401F8000
    size: 0x4000
    initable: true
    filename: "scripts/pydev/flipflop.py"

analog01: Python.PythonPeripheral @ sysbus 0x400D8000
    size: 0x30
    initable: true
    filename: "scripts/pydev/flipflop.py"

analog03: Python.PythonPeripheral @ sysbus 0x400D8034
    size: 0x3fcc
    initable: true
    filename: "scripts/pydev/flipflop.py"

dcdc: Python.PythonPeripheral @ sysbus 0x40080000
    size: 0x4000
    initable: true
    filename: "scripts/pydev/flipflop.py"

gpTimer1: Timers.IMX_GPTimer @ sysbus 0x401EC000
    IRQ -> nvic@100

lpuart1: UART.NXP_LPUART @ sysbus 0x40184000
    IRQ -> nvic@20

lpuart2: UART.NXP_LPUART @ sysbus 0x40188000
    IRQ -> nvic@21

lpuart3: UART.NXP_LPUART @ sysbus 0x4018c000
    IRQ -> nvic@22

lpuart4: UART.NXP_LPUART @ sysbus 0x40190000
    IRQ -> nvic@23

lpuart5: UART.NXP_LPUART @ sysbus 0x40194000
    IRQ -> nvic@24

lpuart6: UART.NXP_LPUART @ sysbus 0x40198000
    IRQ -> nvic@25

lpuart7: UART.NXP_LPUART @ sysbus 0x4019c000
    IRQ -> nvic@26

lpuart8: UART.NXP_LPUART @ sysbus 0x401a0000
    IRQ -> nvic@27

gpio1: GPIOPort.IMXRT_GPIO @ sysbus 0x401B8000
gpio2: GPIOPort.IMXRT_GPIO @ sysbus 0x401BC000
gpio3: GPIOPort.IMXRT_GPIO @ sysbus 0x401C0000
gpio4: GPIOPort.IMXRT_GPIO @ sysbus 0x401C4000
gpio5: GPIOPort.IMXRT_GPIO @ sysbus 0x400C0000
gpio6: GPIOPort.IMXRT_GPIO @ sysbus 0x42000000
gpio7: GPIOPort.IMXRT_GPIO @ sysbus 0x42004000
gpio8: GPIOPort.IMXRT_GPIO @ sysbus 0x42008000
gpio9: GPIOPort.IMXRT_GPIO @ sysbus 0x4200C000
gpio10: GPIOPort.IMXRT_GPIO @ sysbus 0x401C8000

enetIRQs: Miscellaneous.CombinedInput
    numberOfInputs: 4
    -> nvic@114

enet2IRQs: Miscellaneous.CombinedInput
    numberOfInputs: 4
    -> nvic@152

enet: Network.K6xF_Ethernet @ sysbus 0x402D8000
    [TxIRQ, RxIRQ, MiscIRQ, PtpIRQ] -> enetIRQs@[0-3]
    TimerIRQ -> nvic@115

enet2: Network.K6xF_Ethernet @ sysbus 0x402D4000
    [TxIRQ, RxIRQ, MiscIRQ, PtpIRQ] -> enet2IRQs@[0-3]
    TimerIRQ -> nvic@153

flex_spi: SPI.IMXRT_FlexSPI @ {
    sysbus 0x402A8000;
    sysbus new Bus.BusMultiRegistration { address: 0x60000000; size: 0xF000000; region: "ciphertext" }
}

flex_spi2: SPI.IMXRT_FlexSPI @ sysbus 0x402A4000

// alternative way of defining flex_spi2 is presented below:
// in this configuration all reads/writes to the ciphertext region are translated into commands;
// it might not be possible to execute code (XIP) in this setup
// -------------------------------
// flex_spi2: SPI.IMXRT_FlexSPI @ {
//     sysbus 0x402A4000;
//     sysbus new Bus.BusMultiRegistration { address: 0x70000000; size: 0xF000000; region: "ciphertext" }
// }

lpspi1 : SPI.IMXRT_LPSPI @ sysbus 0x40394000

lpspi2 : SPI.IMXRT_LPSPI @ sysbus 0x40398000

lpspi3 : SPI.IMXRT_LPSPI @ sysbus 0x4039C000

lpspi4 : SPI.IMXRT_LPSPI @ sysbus 0x403A0000

adc1: Analog.IMXRT_ADC @ sysbus 0x400C4000
    referenceVoltage: 3.3 // default value that can be overwritten in board platform description
    -> nvic@67

adc2: Analog.IMXRT_ADC @ sysbus 0x400C8000
    referenceVoltage: 3.3 // default value that can be overwritten in board platform description
    -> nvic@68

pwm1: Timers.IMXRT_PWM @ sysbus 0x403DC000

pwm2: Timers.IMXRT_PWM @ sysbus 0x403E0000
    2 -> nvic@137 // Reload IRQ for submodule 0

pwm3: Timers.IMXRT_PWM @ sysbus 0x403E4000

pwm4: Timers.IMXRT_PWM @ sysbus 0x403E8000

sysbus:
    init:
        Tag <0x41400000, 0x414FFFFF> "cpu configuration port"
        Tag <0x41100000, 0x411FFFFF> "m configuration port"
        Tag <0x41000000, 0x410FFFFF> "main configuration port"
        Tag <0x20280000, 0x202FFFFF> "OCRAM - FlexRAM"
        Tag <0x20000000, 0x2007FFFF> "DTCM"
        Tag <0x00200000, 0x0021FFFF> "ROMCP"
        Tag <0x00000000, 0x0007FFFF> "ITCM"
        Tag <0x400FC000, 0x400FFFFF> "CCM(CCM)"
        Tag <0x400FC014, 0x400FC017> "CCM_CBCDR" 0x000A8200
        Tag <0x400FC024, 0x400FC027> "CCM(CSCDR1)" 0x40
        Tag <0x400F8000, 0x400FBFFF> "SRC(SRC)"
        Tag <0x400F4000, 0x400F7FFF> "GPC"
        Tag <0x400EC000, 0x400EFFFF> "DMA_CH_MUX"
        Tag <0x400E8000, 0x400EBFFF> "EDMA"
        Tag <0x400E4000, 0x400E7FFF> "SJC"
        Tag <0x400E0000, 0x400E3FFF> "TSC_DIG"
        Tag <0x400DC000, 0x400DFFFF> "CSU"
        Tag <0x400D8000, 0x400DBFFF> "ANALOG"
        Tag <0x400D8030, 0x400D8033> "analog02" 0x80002001
        Tag <0x400D4000, 0x400D7FFF> "SNVS_HP"
        Tag <0x400D0000, 0x400D3FFF> "WDOG2"
        Tag <0x400BC000, 0x400BFFFF> "WDOG3"
        Tag <0x400B8000, 0x400BBFFF> "WDOG1"
        Tag <0x400B4000, 0x400B7FFF> "EWM"
        Tag <0x400B0000, 0x400B3FFF> "CM7_MXRT (FLEXRAM)"
        Tag <0x400AC000, 0x400AFFFF> "IOMUXC_GPR"
        Tag <0x400A8000, 0x400ABFFF> "IOMUXC_SNVS"
        Tag <0x400A4000, 0x400A7FFF> "IOMUXC_SNVS_GPR"
        Tag <0x40094000, 0x40097FFF> "ACMP"
        Tag <0x40084000, 0x40087FFF> "PIT"
        Tag <0x40080000, 0x40083FFF> "DCDC"
        Tag <0x4007C000, 0x4007FFFF> "AIPS-1 Configuration"
        Tag <0x401FC000, 0x401FFFFF> "KPP"
        Tag <0x401F8000, 0x401FBFFF> "IOMUXC"
        Tag <0x401F4000, 0x401F7FFF> "OCOTP"
        Tag <0x401F0000, 0x401F3FFF> "GPT2"
        Tag <0x401EC000, 0x401EFFFF> "GPT1"
        Tag <0x401E8000, 0x401EBFFF> "QTimer4"
        Tag <0x401E4000, 0x401E7FFF> "QTimer3"
        Tag <0x401E0000, 0x401E3FFF> "QTimer2"
        Tag <0x401DC000, 0x401DFFFF> "QTimer1"
        Tag <0x401D8000, 0x401DBFFF> "FlexCAN3"
        Tag <0x401D4000, 0x401D7FFF> "FlexCAN2"
        Tag <0x401D0000, 0x401D3FFF> "FlexCAN1"
        Tag <0x401B0000, 0x401B3FFF> "FlexIO2"
        Tag <0x401AC000, 0x401AFFFF> "FlexIO1"
        Tag <0x40180000, 0x40183FFF> "ROMCP"
        Tag <0x401AC010, 0x401AC013> "flexio1" 0xfffffff
        Tag <0x4017C000, 0x4017FFFF> "AIPS-2 Configuration"
        Tag <0x402FC000, 0x402FFFFF> "DCP"
        Tag <0x402F0000, 0x402F3FFF> "SEMC"
        Tag <0x402E0000, 0x402E3FFF> "USB(USB)"
        Tag <0x402C4000, 0x402C7FFF> "USDHC2"
        Tag <0x402C0000, 0x402C3FFF> "USDHC1"
        Tag <0x402BC000, 0x402BFFFF> "CSI"
        Tag <0x402B8000, 0x402BBFFF> "LCDIF"
        Tag <0x402B4000, 0x402B7FFF> "PXP"
        Tag <0x4027C000, 0x4027FFFF> "AIPS-3 Configuration"
        Tag <0x403FC000, 0x403FFFFF> "LPI2C4"
        Tag <0x403F8000, 0x403FBFFF> "LPI2C3"
        Tag <0x403F4000, 0x403F7FFF> "LPI2C2"
        Tag <0x403F0000, 0x403F3FFF> "LPI2C1"
        Tag <0x403EC000, 0x403EFFFF> "BEE"
        Tag <0x403D4000, 0x403D7FFF> "ENC4"
        Tag <0x403D0000, 0x403D3FFF> "ENC3"
        Tag <0x403CC000, 0x403CFFFF> "ENC2"
        Tag <0x403C8000, 0x403CBFFF> "ENC1"
        Tag <0x403C4000, 0x403C7FFF> "XBAR3"
        Tag <0x403C0000, 0x403C3FFF> "XBAR2"
        Tag <0x403BC000, 0x403BFFFF> "XBAR1"
        Tag <0x403B8000, 0x403BBFFF> "AOI2"
        Tag <0x403B4000, 0x403B7FFF> "AOI1"
        Tag <0x403B0000, 0x403B3FFF> "ADC_ETC"
        Tag <0x4038C000, 0x4038FFFF> "SAI3"
        Tag <0x40388000, 0x4038BFFF> "SAI2"
        Tag <0x40384000, 0x40387FFF> "SAI1"
        Tag <0x40380000, 0x40383FFF> "SPDIF"
        Tag <0x4037C000, 0x4037FFFF> "AIPS-4 Configuration"
        Tag <0x42020000, 0x42023FFF> "FlexIO3"
        Tag <0x7FC00000, 0x7FFFFFFF> "FlexSPI RX FIFO"
        Tag <0x7F800000, 0x7FBFFFFF> "FlexSPI TX FIFO"
        Tag <0x7F400000, 0x7F7FFFFF> "FlexSPI2 RX FIFO"
        Tag <0x7F000000, 0x7F3FFFFF> "FlexSPI2 TX FIFO"
